<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="160" y2="0" width="0" layer="20"/>
<wire x1="160" y1="0" x2="160" y2="100" width="0" layer="20"/>
<wire x1="160" y1="100" x2="0" y2="100" width="0" layer="20"/>
<wire x1="0" y1="100" x2="0" y2="0" width="0" layer="20"/>
<hole x="3.5" y="5.625" drill="2.8"/>
<hole x="3.5" y="94.375" drill="2.8"/>
<text>General purpose controller</text>
<text>Proportional</text>
<text>Integrator</text>
<text>Double integrator</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>Serge Grop ULISS-ST</text>
<text>Proportional</text>
<text>Integrator</text>
<text>Double integrator</text>
<text>voltage reference</text>
<text>modulation and bias sum</text>
<text>summator</text>
<text>-12/-15V</text>
<text>+12/+15V</text>
</plain>
<libraries>
<library name="rcl">
<packages>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="CT7343">
<description>&lt;b&gt;TANTALUM CAPACITOR&lt;/b&gt;</description>
</package>
<package name="RTRIM3224W">
<description>&lt;b&gt;Trimm resistor&lt;/b&gt; BOURNS&lt;p&gt;
Top Adjust</description>
</package>
<package name="C1210K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1210 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3225</description>
</package>
<package name="0207/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 12 mm</description>
</package>
<package name="C1210">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C050-025X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 2.5 x 7.5 mm</description>
</package>
<package name="RTRIM64X">
<description>&lt;b&gt;Trimm resistor&lt;/b&gt; Spectrol&lt;p&gt;
Cermet MIL-R-22097</description>
</package>
</packages>
</library>
<library name="linear">
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package 8&lt;/b&gt;&lt;br&gt;
NS Package M08A</description>
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-coax">
<packages>
<package name="BU-SMA-V">
<description>FEMALE &lt;b&gt;SMA CONNECTOR&lt;/b&gt;&lt;p&gt;
Radiall&lt;p&gt;
distributor RS 112-3794</description>
</package>
</packages>
</library>
<library name="srinos-lib">
<packages>
<package name="SWITCH">
</package>
<package name="MSOP-RM8">
</package>
</packages>
</library>
<library name="burr-brown">
<description>&lt;b&gt;Burr-Brown Components&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-vg">
<description>&lt;b&gt;VG Connectors (DIN 41612/DIN 41617)&lt;/b&gt;&lt;p&gt;
The library contains devices which allow to place the contacts individually or 
in one or several blocks.&lt;p&gt;
This behavior is indicated by the key words &lt;i&gt;single&lt;/i&gt; and &lt;i&gt;block&lt;/i&gt; in
the respective device descriptions.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MAC32L">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
male, 32 pins, type D, rows AC, grid 5.08 mm&lt;p&gt;
with mounting clip</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO35-7">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2 mm, horizontal, grid 7.62 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="linear" package="SO08" value="OP27D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="linear" package="SO08" value="OP27D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC5" library="linear" package="SO08" value="OP27D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC6" library="linear" package="SO08" value="OP27D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC7" library="linear" package="SO08" value="OP27D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="rcl" package="R0805" value="5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="rcl" package="R0805" value="5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="rcl" package="R0805" value="5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="rcl" package="R0805" value="5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="rcl" package="R0805" value="5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="rcl" package="R0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SWITCH2" library="srinos-lib" package="SWITCH" value="pro"/>
<element name="SWITCH4" library="srinos-lib" package="SWITCH" value="SWITCH"/>
<element name="IC9" library="linear" package="DIL08" value="REF01Z">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC10" library="linear" package="SO08" value="OP27D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="rcl" package="R0805" value="10k +/-0.1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="rcl" package="R0805" value="10k +/-0.1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="rcl" package="CT7343" value="47u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="rcl" package="CT7343" value="47u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC11" library="linear" package="SO08" value="OP27D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="rcl" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="rcl" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SWITCH1" library="srinos-lib" package="SWITCH" value="SWITCH"/>
<element name="R17" library="rcl" package="R0805" value="4k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="rcl" package="R0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C31" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="rcl" package="RTRIM3224W" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="rcl" package="RTRIM3224W" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="rcl" package="RTRIM3224W" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="rcl" package="RTRIM3224W" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="rcl" package="R0805" value="5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="rcl" package="R0805" value="2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="rcl" package="C1210K" value="100µ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C33" library="rcl" package="C1210K" value="100µ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC15" library="linear" package="SO08" value="OP27D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="rcl" package="R0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="rcl" package="R0805" value="2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C34" library="rcl" package="C1210K" value="100µ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C35" library="rcl" package="C1210K" value="100µ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R36" library="rcl" package="R0805" value="3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C36" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C37" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C38" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C39" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C40" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C41" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C42" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C43" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC16" library="linear" package="SO08" value="OP27D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="rcl" package="R0805" value="3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R38" library="rcl" package="R0805" value="3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC17" library="burr-brown" package="SO08" value="OPA177S">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="IC13" library="burr-brown" package="SO08" value="OPA177S">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="X7" library="con-vg" package="MAC32L" value="MAC32L"/>
<element name="R39" library="rcl" package="R0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC14" library="linear" package="SO08" value="OP27D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P" library="rcl" package="RTRIM64X" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="I" library="rcl" package="RTRIM64X" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="II" library="rcl" package="RTRIM64X" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BIAS" library="rcl" package="RTRIM64X" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IN_BUF" library="con-coax" package="BU-SMA-V" value="BU-SMA-V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT_BUF" library="con-coax" package="BU-SMA-V" value="BU-SMA-V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="NOISE" library="con-coax" package="BU-SMA-V" value="BU-SMA-V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MOD_BIAS" library="rcl" package="RTRIM64X" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT_MOD" library="con-coax" package="BU-SMA-V" value="BU-SMA-V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IN_MOD" library="con-coax" package="BU-SMA-V" value="BU-SMA-V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IN" library="con-coax" package="BU-SMA-V" value="BU-SMA-V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT" library="con-coax" package="BU-SMA-V" value="BU-SMA-V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SPST1" library="srinos-lib" package="MSOP-RM8" value="ADG1401">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SPST2" library="srinos-lib" package="MSOP-RM8" value="ADG1402">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SPST3" library="srinos-lib" package="MSOP-RM8" value="ADG1401">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SPST4" library="srinos-lib" package="MSOP-RM8" value="ADG1401">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="rcl" package="RTRIM3224W" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C44" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C45" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RI" library="rcl" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RI1" library="rcl" package="0207/12" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CI" library="rcl" package="C1210" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CI1" library="rcl" package="C050-025X075" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RP1" library="rcl" package="0207/12" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RP" library="rcl" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RG" library="rcl" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RG1" library="rcl" package="0207/12" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RII2" library="rcl" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RII3" library="rcl" package="0207/12" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CII2" library="rcl" package="C050-025X075" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CII3" library="rcl" package="C1210" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RII4" library="rcl" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RII5" library="rcl" package="0207/12" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CII4" library="rcl" package="C1210" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CII5" library="rcl" package="C050-025X075" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="R0805" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="R0805" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC18" library="linear" package="SO08" value="OP27D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC19" library="linear" package="SO08" value="OP27D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C46" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C47" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C49" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C50" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="diode" package="DO35-7" value="1N4148DO35-7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="diode" package="DO35-7" value="1N4148DO35-7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="diode" package="DO35-7" value="1N4148DO35-7"/>
<element name="R*" library="rcl" package="R0805" value=""/>
<element name="R1*" library="rcl" package="R0805" value=""/>
<element name="R34" library="rcl" package="R0805" value="2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32*" library="rcl" package="R0805" value="2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32*2" library="rcl" package="R0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32*3" library="rcl" package="R0805" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl" package="R0805" value="150">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="1"/>
<contactref element="C16" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="C15" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C14" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="C12" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="C11" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="C10" pad="2"/>
<contactref element="C19" pad="-"/>
<contactref element="C20" pad="+"/>
<contactref element="C22" pad="1"/>
<contactref element="C21" pad="2"/>
<contactref element="C28" pad="1"/>
<contactref element="C23" pad="2"/>
<contactref element="C29" pad="1"/>
<contactref element="C24" pad="2"/>
<contactref element="C30" pad="1"/>
<contactref element="C25" pad="2"/>
<contactref element="C31" pad="1"/>
<contactref element="C26" pad="2"/>
<contactref element="IC9" pad="4"/>
<contactref element="C18" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="R15" pad="2"/>
<contactref element="R16" pad="2"/>
<contactref element="C33" pad="2"/>
<contactref element="C35" pad="2"/>
<contactref element="C40" pad="1"/>
<contactref element="C36" pad="2"/>
<contactref element="C41" pad="1"/>
<contactref element="C37" pad="2"/>
<contactref element="C42" pad="1"/>
<contactref element="C38" pad="2"/>
<contactref element="C43" pad="1"/>
<contactref element="C39" pad="2"/>
<contactref element="X7" pad="C32"/>
<contactref element="X7" pad="A32"/>
<contactref element="R39" pad="2"/>
<contactref element="IN_BUF" pad="2"/>
<contactref element="IN_BUF" pad="4"/>
<contactref element="IN_BUF" pad="3"/>
<contactref element="IN_BUF" pad="5"/>
<contactref element="IN_BUF" pad="2"/>
<contactref element="OUT_BUF" pad="2"/>
<contactref element="OUT_BUF" pad="4"/>
<contactref element="OUT_BUF" pad="3"/>
<contactref element="OUT_BUF" pad="5"/>
<contactref element="OUT_BUF" pad="2"/>
<contactref element="NOISE" pad="2"/>
<contactref element="NOISE" pad="4"/>
<contactref element="NOISE" pad="3"/>
<contactref element="NOISE" pad="5"/>
<contactref element="NOISE" pad="2"/>
<contactref element="OUT_MOD" pad="2"/>
<contactref element="OUT_MOD" pad="4"/>
<contactref element="OUT_MOD" pad="3"/>
<contactref element="OUT_MOD" pad="5"/>
<contactref element="OUT_MOD" pad="2"/>
<contactref element="IN_MOD" pad="2"/>
<contactref element="IN_MOD" pad="4"/>
<contactref element="IN_MOD" pad="3"/>
<contactref element="IN_MOD" pad="5"/>
<contactref element="IN_MOD" pad="2"/>
<contactref element="IN" pad="2"/>
<contactref element="IN" pad="4"/>
<contactref element="IN" pad="3"/>
<contactref element="IN" pad="5"/>
<contactref element="IN" pad="2"/>
<contactref element="OUT" pad="2"/>
<contactref element="OUT" pad="4"/>
<contactref element="OUT" pad="3"/>
<contactref element="OUT" pad="5"/>
<contactref element="OUT" pad="2"/>
<contactref element="SPST1" pad="P$3"/>
<contactref element="SPST2" pad="P$3"/>
<contactref element="SPST3" pad="P$3"/>
<contactref element="SPST4" pad="P$3"/>
<contactref element="C45" pad="1"/>
<contactref element="C44" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R21" pad="1"/>
<contactref element="C46" pad="2"/>
<contactref element="C49" pad="1"/>
<contactref element="C47" pad="2"/>
<contactref element="C50" pad="1"/>
<contactref element="D3" pad="A"/>
<contactref element="I" pad="1"/>
<contactref element="II" pad="1"/>
<contactref element="P" pad="1"/>
<contactref element="SWITCH2" pad="P$1"/>
<contactref element="SWITCH1" pad="P$1"/>
<contactref element="SWITCH4" pad="P$1"/>
<contactref element="R32*2" pad="2"/>
</signal>
<signal name="+12V">
<contactref element="C16" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C19" pad="+"/>
<contactref element="C21" pad="1"/>
<contactref element="C23" pad="1"/>
<contactref element="C24" pad="1"/>
<contactref element="C25" pad="1"/>
<contactref element="C26" pad="1"/>
<contactref element="IC2" pad="7"/>
<contactref element="IC3" pad="7"/>
<contactref element="IC5" pad="7"/>
<contactref element="IC7" pad="7"/>
<contactref element="IC6" pad="7"/>
<contactref element="IC9" pad="2"/>
<contactref element="C18" pad="1"/>
<contactref element="IC10" pad="7"/>
<contactref element="IC11" pad="7"/>
<contactref element="IC17" pad="7"/>
<contactref element="IC15" pad="7"/>
<contactref element="IC16" pad="7"/>
<contactref element="X7" pad="A26"/>
<contactref element="C36" pad="1"/>
<contactref element="C37" pad="1"/>
<contactref element="C38" pad="1"/>
<contactref element="C39" pad="1"/>
<contactref element="IC14" pad="7"/>
<contactref element="SPST1" pad="P$4"/>
<contactref element="SPST2" pad="P$4"/>
<contactref element="SPST3" pad="P$4"/>
<contactref element="SPST4" pad="P$4"/>
<contactref element="C44" pad="1"/>
<contactref element="R23" pad="2"/>
<contactref element="IC13" pad="7"/>
<contactref element="R22" pad="2"/>
<contactref element="R26" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="R27" pad="2"/>
<contactref element="C47" pad="1"/>
<contactref element="C46" pad="1"/>
<contactref element="IC18" pad="7"/>
<contactref element="IC19" pad="7"/>
<contactref element="SWITCH2" pad="P$3"/>
<contactref element="SWITCH1" pad="P$3"/>
<contactref element="SWITCH4" pad="P$3"/>
</signal>
<signal name="-12V">
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C20" pad="-"/>
<contactref element="C22" pad="2"/>
<contactref element="C28" pad="2"/>
<contactref element="C29" pad="2"/>
<contactref element="C30" pad="2"/>
<contactref element="C31" pad="2"/>
<contactref element="IC2" pad="4"/>
<contactref element="IC3" pad="4"/>
<contactref element="IC5" pad="4"/>
<contactref element="IC7" pad="4"/>
<contactref element="IC6" pad="4"/>
<contactref element="IC10" pad="4"/>
<contactref element="IC11" pad="4"/>
<contactref element="IC17" pad="4"/>
<contactref element="IC13" pad="4"/>
<contactref element="IC15" pad="4"/>
<contactref element="IC16" pad="4"/>
<contactref element="X7" pad="A24"/>
<contactref element="C40" pad="2"/>
<contactref element="C41" pad="2"/>
<contactref element="C42" pad="2"/>
<contactref element="C43" pad="2"/>
<contactref element="IC14" pad="4"/>
<contactref element="SPST1" pad="P$7"/>
<contactref element="SPST2" pad="P$7"/>
<contactref element="SPST3" pad="P$7"/>
<contactref element="SPST4" pad="P$7"/>
<contactref element="C45" pad="2"/>
<contactref element="C49" pad="2"/>
<contactref element="C50" pad="2"/>
<contactref element="IC18" pad="4"/>
<contactref element="IC19" pad="4"/>
</signal>
<signal name="IN_BUF_OUT">
<contactref element="IC2" pad="6"/>
<contactref element="IC2" pad="2"/>
<contactref element="IN_BUF" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R6" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="IC7" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="R33" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="ERR_BUF">
<contactref element="IC14" pad="3"/>
<contactref element="IC7" pad="6"/>
<contactref element="R10" pad="1"/>
<contactref element="D2" pad="A"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="IC10" pad="3"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="IC10" pad="2"/>
<contactref element="R18" pad="1"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="+10V">
<contactref element="MOD_BIAS" pad="3"/>
<contactref element="R18" pad="2"/>
<contactref element="IC9" pad="6"/>
<contactref element="BIAS" pad="3"/>
</signal>
<signal name="-10V">
<contactref element="IC10" pad="6"/>
<contactref element="R19" pad="1"/>
<contactref element="BIAS" pad="1"/>
<contactref element="MOD_BIAS" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="IC5" pad="2"/>
<contactref element="RP" pad="2"/>
<contactref element="RP1" pad="2"/>
<contactref element="RG" pad="1"/>
<contactref element="RG1" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="R2" pad="1"/>
<contactref element="IC5" pad="3"/>
</signal>
<signal name="N$18">
<contactref element="IC3" pad="3"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="R15" pad="1"/>
<contactref element="IC17" pad="3"/>
</signal>
<signal name="N$25">
<contactref element="R16" pad="1"/>
<contactref element="IC13" pad="3"/>
</signal>
<signal name="N$26">
<contactref element="IC7" pad="3"/>
<contactref element="R21" pad="2"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="N$34">
<contactref element="IC17" pad="8"/>
<contactref element="R22" pad="1"/>
</signal>
<signal name="N$32">
<contactref element="IC5" pad="8"/>
<contactref element="R27" pad="1"/>
</signal>
<signal name="N$46">
<contactref element="IC13" pad="8"/>
<contactref element="R23" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="IC6" pad="6"/>
<contactref element="R13" pad="2"/>
<contactref element="C17" pad="2"/>
</signal>
<signal name="V_REF">
<contactref element="R13" pad="1"/>
<contactref element="R24" pad="1"/>
<contactref element="C33" pad="1"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$50">
<contactref element="C17" pad="1"/>
<contactref element="IC6" pad="2"/>
<contactref element="R24" pad="2"/>
</signal>
<signal name="N$51">
<contactref element="IC6" pad="3"/>
<contactref element="BIAS" pad="2"/>
</signal>
<signal name="N$47">
<contactref element="R33" pad="2"/>
<contactref element="NOISE" pad="1"/>
</signal>
<signal name="N$52">
<contactref element="IC15" pad="6"/>
<contactref element="R25" pad="2"/>
<contactref element="C34" pad="2"/>
</signal>
<signal name="N$53">
<contactref element="C34" pad="1"/>
<contactref element="IC15" pad="2"/>
<contactref element="R35" pad="2"/>
</signal>
<signal name="N$54">
<contactref element="IC15" pad="3"/>
<contactref element="MOD_BIAS" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="R37" pad="2"/>
<contactref element="IN_MOD" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="IC16" pad="2"/>
<contactref element="R37" pad="1"/>
<contactref element="R36" pad="1"/>
<contactref element="R38" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="IC16" pad="6"/>
<contactref element="R38" pad="1"/>
<contactref element="OUT_MOD" pad="1"/>
<contactref element="IC19" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="IC16" pad="3"/>
<contactref element="R39" pad="1"/>
</signal>
<signal name="V_REF_MOD">
<contactref element="R25" pad="1"/>
<contactref element="R35" pad="1"/>
<contactref element="C35" pad="1"/>
<contactref element="R36" pad="2"/>
</signal>
<signal name="ERR_BUF_OUT">
<contactref element="IC14" pad="6"/>
<contactref element="IC14" pad="2"/>
<contactref element="OUT_BUF" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="RP" pad="1"/>
<contactref element="RP1" pad="1"/>
<contactref element="P" pad="2"/>
</signal>
<signal name="N$30">
<contactref element="RI" pad="1"/>
<contactref element="RI1" pad="1"/>
<contactref element="I" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="RII2" pad="1"/>
<contactref element="RII3" pad="1"/>
<contactref element="II" pad="2"/>
</signal>
<signal name="SI">
<contactref element="SPST1" pad="P$1"/>
<contactref element="IC3" pad="2"/>
<contactref element="RI" pad="2"/>
<contactref element="RI1" pad="2"/>
<contactref element="CI" pad="1"/>
<contactref element="CI1" pad="1"/>
</signal>
<signal name="DI">
<contactref element="SPST1" pad="P$8"/>
<contactref element="IC3" pad="6"/>
<contactref element="R8" pad="2"/>
<contactref element="CI" pad="2"/>
<contactref element="CI1" pad="2"/>
</signal>
<signal name="INI">
<contactref element="SPST1" pad="P$6"/>
<contactref element="SWITCH4" pad="P$2"/>
</signal>
<signal name="N$3">
<contactref element="IC3" pad="8"/>
<contactref element="R26" pad="1"/>
</signal>
<signal name="DG">
<contactref element="SPST2" pad="P$8"/>
<contactref element="IC11" pad="6"/>
<contactref element="R34" pad="1"/>
</signal>
<signal name="SG">
<contactref element="SPST2" pad="P$1"/>
<contactref element="I" pad="3"/>
<contactref element="II" pad="3"/>
<contactref element="P" pad="3"/>
</signal>
<signal name="ING">
<contactref element="SPST2" pad="P$6"/>
<contactref element="SWITCH2" pad="P$2"/>
</signal>
<signal name="INII">
<contactref element="SPST3" pad="P$6"/>
<contactref element="SPST4" pad="P$6"/>
<contactref element="SWITCH1" pad="P$2"/>
</signal>
<signal name="SII2">
<contactref element="SPST4" pad="P$1"/>
<contactref element="IC13" pad="2"/>
<contactref element="RII4" pad="2"/>
<contactref element="RII5" pad="2"/>
<contactref element="CII4" pad="1"/>
<contactref element="CII5" pad="1"/>
</signal>
<signal name="DII2">
<contactref element="SPST4" pad="P$8"/>
<contactref element="IC18" pad="3"/>
<contactref element="IC13" pad="6"/>
<contactref element="R17" pad="2"/>
<contactref element="R1*" pad="2"/>
</signal>
<signal name="SII1">
<contactref element="SPST3" pad="P$1"/>
<contactref element="IC17" pad="2"/>
<contactref element="RII2" pad="2"/>
<contactref element="RII3" pad="2"/>
<contactref element="CII3" pad="1"/>
<contactref element="CII2" pad="1"/>
</signal>
<signal name="DII1">
<contactref element="SPST3" pad="P$8"/>
<contactref element="IC17" pad="6"/>
<contactref element="RII4" pad="1"/>
<contactref element="RII5" pad="1"/>
<contactref element="R*" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="IC7" pad="1"/>
<contactref element="R14" pad="3"/>
</signal>
<signal name="N$28">
<contactref element="IC7" pad="8"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R23" pad="3"/>
<contactref element="IC13" pad="1"/>
</signal>
<signal name="N$31">
<contactref element="R22" pad="3"/>
<contactref element="IC17" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="R26" pad="3"/>
<contactref element="IC3" pad="1"/>
</signal>
<signal name="N$33">
<contactref element="R27" pad="3"/>
<contactref element="IC5" pad="1"/>
</signal>
<signal name="N$37">
<contactref element="RG" pad="2"/>
<contactref element="RG1" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="IC5" pad="6"/>
</signal>
<signal name="N$38">
<contactref element="X7" pad="C26"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="DI_BUF_OUT">
<contactref element="IC18" pad="2"/>
<contactref element="IC18" pad="6"/>
<contactref element="X7" pad="C24"/>
</signal>
<signal name="N$6">
<contactref element="X7" pad="C20"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="BIAS_MOD_BUF_OUT">
<contactref element="X7" pad="C18"/>
<contactref element="IC19" pad="6"/>
<contactref element="IC19" pad="2"/>
</signal>
<signal name="N$39">
<contactref element="D1" pad="C"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="N$40">
<contactref element="CII3" pad="2"/>
<contactref element="CII2" pad="2"/>
<contactref element="R*" pad="1"/>
</signal>
<signal name="N$42">
<contactref element="CII4" pad="2"/>
<contactref element="R1*" pad="1"/>
<contactref element="CII5" pad="2"/>
</signal>
<signal name="N$41">
<contactref element="IC11" pad="2"/>
<contactref element="R34" pad="2"/>
<contactref element="R32*" pad="1"/>
</signal>
<signal name="N$43">
<contactref element="IN" pad="1"/>
<contactref element="IC2" pad="3"/>
<contactref element="R32*" pad="2"/>
<contactref element="R32*3" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="R32*2" pad="1"/>
<contactref element="R32*3" pad="2"/>
<contactref element="IC11" pad="3"/>
</signal>
<signal name="N$2">
</signal>
<signal name="N$12">
</signal>
<signal name="N$13">
<contactref element="OUT" pad="1"/>
<contactref element="D3" pad="C"/>
<contactref element="R1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
